| Samsung Internal API reference 2.0

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- File List
- Globals

File List
Here is a list of all documented files with brief descriptions:
[detail level 1 2 3]

▼ core |
error.h |
itimer.h |
lseek.h |
mman.h |
stat.h |
tbt.h |
▼ driver |
▼ co |
cache_object.h |
▼ mem |
phys.h |
▼ smc |
smc.h |
▼ sys |
credentials.h | Definitions for credentials
ioctl.h | Ioctl declaration
mman.h | Memory mapping declarations
socket.h | Support socket routines
stat.h | File status syscalls
types.h | Wrapper for kernel types.h header
un.h | Definitions for UNIX domain sockets
▼ uuid |
uuid.h | UUID management helpers
alloca.h | Alloca implementation
assert.h | Assertion support
cache.h | Cache maintenance
ctype.h | Critical sections support
driver.h | User-space driver API declarations
errno.h | System error numbers
fcntl.h | Fcntl declarations
fops.h |
inttypes.h | Integer type declrations
irs.h | Integrity Report System
ld_debug.h |
limits.h | Implementation-defined constants
malloc.h | Memory allocation definitions
math.h | Math library
mqueue.h | POSIX message queue declarations
print_no_alloc.h |
protocol_errors.h | ISocket Protocol error extended codes definitions
pthread.h | POSIX compatible thread library
rpmb.h | TEESL: RPMB API
sched.h | Scheduler syscalls
scma.h | Secure Contiguous memory allocator API
stdint.h |
stdio.h | Standard I/O
stdlib.h | Standard library header
string.h | String manipulation funcitons
tee_error.h | Manipulation with errno and TEE error
tee_i2c.h | TEE I2C public API
tee_internal_se_api.h |
tee_interrupt.h | Interrupt syscalls
tee_isocket.h | GP iSockets interface (GPD_SPE_100)
tee_nfc.h | TEE NFC public API
tee_smc.h | TEE SMC public API
tee_spi.h | TEE SPI public API
tee_ta_destructor.h | Driver destructor registration header
tee_tcpsocket.h | GP iSockets TCP API header (GPD_SPE_101)
tee_tlssocket.h | GP iSockets TLS API (GPD_SPE_103)
tee_udpsocket.h | GP iSockets UDP API header (GPD_SPE_102)
tees_critical.h | Critical sections support
tees_el2if.h | EL2 interface support
tees_extension.h | Samsung's extension of TEE internal API
tees_hwcrypto_buf.h | Lock or Unlock HW crypto buffer
tees_internal_api.h |
tees_iwt.h | Samsung IWT API header
tees_kdf.h | KDF API
tees_rot.h | ROT API
tees_secure_object.h | Secure Objects API
tees_ssapi.h | Samsung SMC APIs
tees_tui.h | The Trusted User Interface API permits the display of screens to the user and achieves three objectives:
tees_wrapped_with_rek.h | Wrapped with REK API
time.h | Time header
tui.h | The Trusted User Interface API permits the display of screens to the user and achieves three objectives:
udf.h | User-space Driver Framework declarations
udf_interrupt.h |
unistd.h | Unistd header