| Samsung Internal API reference 2.0

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- File List
- Globals

Typedefs | Enumerations | Functions
tees_iwt.h File Reference

Samsung IWT API header. More...

Go to the source code of this file.

## Typedefs
typedef struct __TEES_IwtHandle * | TEES_IwtHandle
| Handle representing active IWT connection. Must be treated as opaque structure.

## Enumerations
enum | { TEES_IWT_LISTENER_NAME_MAX_LENGTH = 91 }
| TEES_IWT_LISTENER_NAME_MAX_LENGTH. More...

## Functions
TEE_Result | TEES_IwtOpenChannel (const char *listenerName, TEES_IwtHandle *iwtCtx)
| Open interworld transport (IWT) connection (channel) to the NWd Listener "listenerName". More...
TEE_Result | TEES_IwtWrite (TEES_IwtHandle iwtCtx, const void *buf, uint32_t *length)
| Write `length` bytes from `buf` to the active IWT connection `iwtCtx`. More...
TEE_Result | TEES_IwtRead (TEES_IwtHandle iwtCtx, void *buf, uint32_t *length)
| Read `length` bytes to `buf` from the active IWT connection `iwtCtx`. More...
TEE_Result | TEES_IwtCloseChannel (TEES_IwtHandle iwtCtx)
| Close active IWT connection `iwtCtx`. More...

## Detailed Description

Samsung IWT API header.

Copyright
  (C) 2012-2019, Samsung Electronics Co., Ltd.