| Samsung Internal API reference 2.0

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- File List
- Globals

Enumerations | Functions
rpmb.h File Reference

TEESL: RPMB API. More...

Go to the source code of this file.

## Enumerations
enum | { RPMB_TYPE_BLOCK = 0, RPMB_TYPE_BYTE = 1 }
| RPMB I/O type. More...

## Functions
TEE_Result | TEES_RPMBRead (uint32_t partition, uint32_t offset, uint8_t *data, uint32_t size, uint8_t type)
| Read data from RPMB Storage. More...
TEE_Result | TEES_RPMBWrite (uint32_t partition, uint32_t offset, const uint8_t *data, uint32_t size, uint8_t type)
| Write data to RPMB Storage. More...
TEE_Result | TEES_RPMBCheckEnable (void)
| Check RPMB availability. More...

## Detailed Description

TEESL: RPMB API.

Copyright
  (C) 2012-2019, Samsung Electronics Co., Ltd.