| Samsung Internal API reference 2.0

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
__TEE_SEAID

## Data Fields
uint8_t * | buffer
uint32_t | bufferLen

## Detailed Description

This type is used to pass the AID of the Applet that a TA wants to communicate with.

## Field Documentation

uint8_t* __TEE_SEAID::buffer

the value of the applet’s AID

uint32_t __TEE_SEAID::bufferLen

length of the applet’s AID