| Samsung Internal API reference 2.0

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
__TEE_SC_OID

## Data Fields
uint8_t * | buffer
uint32_t | bufferLen

## Detailed Description

This type defines the type of protocol which shall be used for the secure channel.

## Field Documentation

uint8_t* __TEE_SC_OID::buffer

the value of the OID

uint32_t __TEE_SC_OID::bufferLen

length of the SC OID