| Samsung Internal API reference 2.0

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- File List
- Globals

Data Structures | Typedefs | Enumerations | Variables
tee_udpsocket.h File Reference

GP iSockets UDP API header (GPD_SPE_102) More...

Go to the source code of this file.

## Data Structures
struct | TEE_udpSocket_Setup_s
| UDP Setup structure. More...
struct | TEE_udpSocket_Change_s
| UDP change addr and port IOCTL structure. TEE_UDP_CHANGE* functions are implementation as synonims. Both server_addr and server_port must be provided for either call. In case of error returned Client should try to open new socket as usual. More...

## Typedefs
typedef struct TEE_udpSocket_Setup_s | TEE_udpSocket_Setup
| UDP Setup structure.
typedef struct TEE_udpSocket_Change_s | TEE_udpSocket_Change
| UDP change addr and port IOCTL structure. TEE_UDP_CHANGE* functions are implementation as synonims. Both server_addr and server_port must be provided for either call. In case of error returned Client should try to open new socket as usual.

## Enumerations
enum | { TEE_ISOCKET_UDP_API_VERSION = 0x01000000 }
| UDP iSocket API version. Used to enshure API structures matching. More...
enum | { TEE_ISOCKET_PROTOCOLID_UDP = 0x66 }
| UDP Protocol identifier. More...
enum | { TEE_ISOCKET_UDP_WARNING_UNKNOWN_OUT_OF_BAND = 0xF1020002 }
| UDP Instance specific errors. More...
enum | { TEE_UDP_CHANGEADDR = 0x66000001, TEE_UDP_CHANGEPORT = 0x66000002 }
| UDP IOCTL codes.

## Variables
const TEE_iSocket *const | TEE_udpSocket
| Public UDP instance pointer.

## Detailed Description

GP iSockets UDP API header (GPD_SPE_102)

Copyright
  (C) 2012-2019, Samsung Electronics Co., Ltd.