| Samsung Internal API reference 2.0

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- File List
- Globals

Macros
error.h File Reference
Auxiliary API

Go to the source code of this file.

## Macros
#define | EPERM 1 /* Operation not permitted */
#define | ENOENT 2 /* No such file or directory */
#define | ESRCH 3 /* No such process */
#define | EINTR 4 /* Interrupted system call */
#define | EIO 5 /* I/O error */
#define | ENXIO 6 /* No such device or address */
#define | E2BIG 7 /* Argument list too long */
#define | ENOEXEC 8 /* Exec format error */
#define | EBADF 9 /* Bad file number */
#define | ECHILD 10 /* No child processes */
#define | EAGAIN 11 /* Try again */
#define | ENOMEM 12 /* Out of memory */
#define | EACCES 13 /* Permission denied */
#define | EFAULT 14 /* Bad address */
#define | ENOTBLK 15 /* Block device required */
#define | EBUSY 16 /* Device or resource busy */
#define | EEXIST 17 /* File exists */
#define | EXDEV 18 /* Cross-device link */
#define | ENODEV 19 /* No such device */
#define | ENOTDIR 20 /* Not a directory */
#define | EISDIR 21 /* Is a directory */
#define | EINVAL 22 /* Invalid argument */
#define | ENFILE 23 /* File table overflow */
#define | EMFILE 24 /* Too many open files */
#define | ENOTTY 25 /* Not a typewriter */
#define | ETXTBSY 26 /* Text file busy */
#define | EFBIG 27 /* File too large */
#define | ENOSPC 28 /* No space left on device */
#define | ESPIPE 29 /* Illegal seek */
#define | EROFS 30 /* Read-only file system */
#define | EMLINK 31 /* Too many links */
#define | EPIPE 32 /* Broken pipe */
#define | EDOM 33 /* Math argument out of domain of func */
#define | ERANGE 34 /* Math result not representable */
#define | EDEADLK 35 /* Resource deadlock would occur */
#define | ENAMETOOLONG 36 /* File name too long */
#define | ENOLCK 37 /* No record locks available */
#define | ENOSYS 38 /* Function not implemented */
#define | ENOTEMPTY 39 /* Directory not empty */
#define | ELOOP 40 /* Too many symbolic links encountered */
#define | EWOULDBLOCK EAGAIN /* Operation would block */
#define | ENOMSG 42 /* No message of desired type */
#define | EIDRM 43 /* Identifier removed */
#define | ECHRNG 44 /* Channel number out of range */
#define | EL2NSYNC 45 /* Level 2 not synchronized */
#define | EL3HLT 46 /* Level 3 halted */
#define | EL3RST 47 /* Level 3 reset */
#define | ELNRNG 48 /* Link number out of range */
#define | EUNATCH 49 /* Protocol driver not attached */
#define | ENOCSI 50 /* No CSI structure available */
#define | EL2HLT 51 /* Level 2 halted */
#define | EBADE 52 /* Invalid exchange */
#define | EBADR 53 /* Invalid request descriptor */
#define | EXFULL 54 /* Exchange full */
#define | ENOANO 55 /* No anode */
#define | EBADRQC 56 /* Invalid request code */
#define | EBADSLT 57 /* Invalid slot */
#define | EDEADLOCK EDEADLK
#define | EBFONT 59 /* Bad font file format */
#define | ENOSTR 60 /* Device not a stream */
#define | ENODATA 61 /* No data available */
#define | ETIME 62 /* Timer expired */
#define | ENOSR 63 /* Out of streams resources */
#define | ENONET 64 /* Machine is not on the network */
#define | ENOPKG 65 /* Package not installed */
#define | EREMOTE 66 /* Object is remote */
#define | ENOLINK 67 /* Link has been severed */
#define | EADV 68 /* Advertise error */
#define | ESRMNT 69 /* Srmount error */
#define | ECOMM 70 /* Communication error on send */
#define | EPROTO 71 /* Protocol error */
#define | EMULTIHOP 72 /* Multihop attempted */
#define | EDOTDOT 73 /* RFS specific error */
#define | EBADMSG 74 /* Not a data message */
#define | EOVERFLOW 75 /* Value too large for defined data type */
#define | ENOTUNIQ 76 /* Name not unique on network */
#define | EBADFD 77 /* File descriptor in bad state */
#define | EREMCHG 78 /* Remote address changed */
#define | ELIBACC 79 /* Can not access a needed shared library */
#define | ELIBBAD 80 /* Accessing a corrupted shared library */
#define | ELIBSCN 81 /* .lib section in a.out corrupted */
#define | ELIBMAX 82 /* Attempting to link in too many shared libraries */
#define | ELIBEXEC 83 /* Cannot exec a shared library directly */
#define | EILSEQ 84 /* Illegal byte sequence */
#define | ERESTART 85 /* Interrupted system call should be restarted */
#define | ESTRPIPE 86 /* Streams pipe error */
#define | EUSERS 87 /* Too many users */
#define | ENOTSOCK 88 /* Socket operation on non-socket */
#define | EDESTADDRREQ 89 /* Destination address required */
#define | EMSGSIZE 90 /* Message too long */
#define | EPROTOTYPE 91 /* Protocol wrong type for socket */
#define | ENOPROTOOPT 92 /* Protocol not available */
#define | EPROTONOSUPPORT 93 /* Protocol not supported */
#define | ESOCKTNOSUPPORT 94 /* Socket type not supported */
#define | EOPNOTSUPP 95 /* Operation not supported on transport endpoint */
#define | EPFNOSUPPORT 96 /* Protocol family not supported */
#define | EAFNOSUPPORT 97 /* Address family not supported by protocol */
#define | EADDRINUSE 98 /* Address already in use */
#define | EADDRNOTAVAIL 99 /* Cannot assign requested address */
#define | ENETDOWN 100 /* Network is down */
#define | ENETUNREACH 101 /* Network is unreachable */
#define | ENETRESET 102 /* Network dropped connection because of reset */
#define | ECONNABORTED 103 /* Software caused connection abort */
#define | ECONNRESET 104 /* Connection reset by peer */
#define | ENOBUFS 105 /* No buffer space available */
#define | EISCONN 106 /* Transport endpoint is already connected */
#define | ENOTCONN 107 /* Transport endpoint is not connected */
#define | ESHUTDOWN 108 /* Cannot send after transport endpoint shutdown */
#define | ETOOMANYREFS 109 /* Too many references: cannot splice */
#define | ETIMEDOUT 110 /* Connection timed out */
#define | ECONNREFUSED 111 /* Connection refused */
#define | EHOSTDOWN 112 /* Host is down */
#define | EHOSTUNREACH 113 /* No route to host */
#define | EALREADY 114 /* Operation already in progress */
#define | EINPROGRESS 115 /* Operation now in progress */
#define | ESTALE 116 /* Stale file handle */
#define | EUCLEAN 117 /* Structure needs cleaning */
#define | ENOTNAM 118 /* Not a XENIX named type file */
#define | ENAVAIL 119 /* No XENIX semaphores available */
#define | EISNAM 120 /* Is a named type file */
#define | EREMOTEIO 121 /* Remote I/O error */
#define | EDQUOT 122 /* Quota exceeded */
#define | ECANCELED 125 /* Operation canceled */
#define | ENOKEY 126 /* Required key not available */
#define | EKEYREJECTED 127 /* Key was rejected by service */
#define | ENOTRECOVERABLE 131 /* State not recoverable */